{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":12,"rows_kept":3,"merged":[[1,3,1,5]],"flags":["formulas_cached_only"]}
[null,"序号","设备名称","设备单价(万元)","拟购置数量","项目名称   （格式：修购项目-平台名称，国重专项-设备名称，或项目名称）","是否具备安装设备的环境条件","是否具备使用设备的专业人员","是否具备维护设备运行的经费和条件","设备预期使用频率\n（预期年度使用时长、次数/年度设计使用时长、次数）","设备主要规格参数","购置设备的必要性"]
[]
["8",1,"液质联用（LC-MS）离子阱质谱",320,1,null,"是","是","是",null,"Q-TOF离子的质量精度一般在测定一级质谱（MS）外标条件下是10ppm, 内标校正条件下是3-5ppm；其二级质谱的质量精度外标条件下为20-30ppm；因此所有的TOF实际分析时都必须实时校正来保证测定的质量精确性。这是Exactive Plus比TOF的优势之一。测定的质量精度都在1ppm以内。此外，在Exactive Plus上，得到的二级质量精确度都能保证在1ppm以内，为更好的定性提供保证。","应用于相关研究领域研究中复杂蛋白质混合物的分析，代谢组学和脂质组学研究等。包括未知肽段的筛选、测序；肽质量指纹图谱测定；蛋白质分子量测定；高通量蛋白质表达谱测定；使用标记或非标记方法进行相对和绝对蛋白质组学定量研究，从而发现疾病或其它重要生理过程相关的生物标志物，寻找药物作用靶点；天然产物鉴定、新药发现、优化与改造等研究，满足研究所诸多科研任务与研究方向的多层次需求"]